Hadronic Isolation Cut

0 2 4 6 8 10 12

Efficiency

0.835

0.84

0.845

0.85

0.855

0.86

Efficiency vs Hadronic isolation cut for rate = 800 Hz